|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Line | Item | Quantity | Unit | Description | Price | Proposal | Call Order | Agency ID |
| 10 | 201000 | 1 | LS | CLEARING AND GRUBBING |  | 4101030 | 1 | NMDOT |
| 20 | 209000 | 16 | MILE | BLADING AND RESHAPING |  | 4101030 | 1 | NMDOT |
| 30 | 301000 | 160400 | S.Y. | FULL DEPTH RECLAMATION |  | 4101030 | 1 | NMDOT |
| 40 | 301005 | 1710 | TON | BITUMINOUS RECYCLING AGENT |  | 4101030 | 1 | NMDOT |
| 50 | 301015 | 740 | TON | MINERAL FILLER |  | 4101030 | 1 | NMDOT |
| 60 | 301016 | 1680 | C.Y. | CORRECTIVE RAP |  | 4101030 | 1 | NMDOT |
| 70 | 403705 | 3460 | TON | WARM MIX OPEN-GRADED FRICTION COURSE COMPLETE |  | 4101030 | 1 | NMDOT |
| 80 | 405000 | 2100 | S.Y. | DETOUR PAVEMENT CONSTRUCTION |  | 4101030 | 1 | NMDOT |
| 90 | 407000 | 104 | TON | ASPHALT MATERIAL FOR TACK COAT |  | 4101030 | 1 | NMDOT |
| 100 | 414000 | 321200 | SYIN | COLD MILLING (ASPHALT) |  | 4101030 | 1 | NMDOT |
| 110 | 424004 | 17960 | TON | WMA SP-IV COMPLETE |  | 4101030 | 1 | NMDOT |
| 120 | 570024 | 24 | L.F. | 24" CULVERT PIPE |  | 4101030 | 1 | NMDOT |
| 130 | 570036 | 70 | L.F. | 36" CULVERT PIPE |  | 4101030 | 1 | NMDOT |
| 140 | 570048 | 332 | L.F. | 48" CULVERT PIPE |  | 4101030 | 1 | NMDOT |
| 150 | 570049 | 8 | EACH | 48" CULVERT PIPE END SECTION |  | 4101030 | 1 | NMDOT |
| 160 | 601000 | 1 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  | 4101030 | 1 | NMDOT |
| 170 | 602000 | 160 | C.Y. | RIPRAP CLASS A |  | 4101030 | 1 | NMDOT |
| 180 | 602010 | 440 | C.Y. | RIPRAP CLASS B |  | 4101030 | 1 | NMDOT |
| 190 | 606001 | 237.5 | L.F. | SINGLE FACE W-BEAM GUARDRAIL |  | 4101030 | 1 | NMDOT |
| 200 | 606051 | 6 | EACH | END TREATMENT TL-3 END TERMINAL |  | 4101030 | 1 | NMDOT |
| 210 | 606061 | 287.5 | L.F. | DRAINAGE STRUCTURE PROTECTION SYSTEM |  | 4101030 | 1 | NMDOT |
| 220 | 606610 | 970 | L.F. | TCWB RETAINED BY THE CONTRACTOR (10') |  | 4101030 | 1 | NMDOT |
| 230 | 606619 | 6010 | L.F. | RESETTING OF TCWB (10') |  | 4101030 | 1 | NMDOT |
| 240 | 607004 | 85000 | L.F. | BARBED WIRE FENCE 4' |  | 4101030 | 1 | NMDOT |
| 250 | 607015 | 400 | EACH | BRACES/CORNER POSTS |  | 4101030 | 1 | NMDOT |
| 260 | 607316 | 9 | EACH | STANDARD GATE, 16' |  | 4101030 | 1 | NMDOT |
| 270 | 607318 | 1 | EACH | STANDARD GATE, 18' |  | 4101030 | 1 | NMDOT |
| 280 | 607320 | 2 | EACH | STANDARD GATE, 20' |  | 4101030 | 1 | NMDOT |
| 290 | 607444 | 1 | EACH | CHAIN LINK GATE, 4' SPAN X 4' RISE |  | 4101030 | 1 | NMDOT |
| 300 | 613000 | 1 | LS | CLEANING CULVERTS AND DRAINAGE STRUCTURES |  | 4101030 | 1 | NMDOT |
| 310 | 618000 | 1 | LS | TRAFFIC CONTROL MANAGEMENT |  | 4101030 | 1 | NMDOT |
| 320 | 618011 | 1 | LS | PUBLIC AWARENESS | 5000 | 4101030 | 1 | NMDOT |
| 330 | 621000 | 1 | LS | MOBILIZATION |  | 4101030 | 1 | NMDOT |
| 340 | 631000 | 84700 | L.F. | RUMBLE STRIPS |  | 4101030 | 1 | NMDOT |
| 350 | 632020 | 1 | ACRE | CLASS C SEEDING |  | 4101030 | 1 | NMDOT |
| 360 | 701000 | 740 | S.F. | PANEL SIGNS |  | 4101030 | 1 | NMDOT |
| 370 | 701100 | 1100 | L.F. | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS |  | 4101030 | 1 | NMDOT |
| 380 | 701101 | 11 | EACH | MULTI-DIRECTIONAL SLIP BASE POSTS FOR ALUMINUM PANEL SIGNS | 4101030 | 1 | NMDOT |
| 390 | 702000 | 41 | S.F. | CONSTRUCTION SIGNING |  | 4101030 | 1 | NMDOT |
| 400 | 702100 | 46 | L.F. | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING |  | 4101030 | 1 | NMDOT |
| 410 | 702101 | 4 | EACH | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING | 4101030 | 1 | NMDOT |
| 420 | 702610 | 2 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  | 4101030 | 1 | NMDOT |
| 430 | 702612 | 2 | EACH | PORTABLE FLOODLIGHT SYSTEM |  | 4101030 | 1 | NMDOT |
| 440 | 702710 | 1 | EACH | MOBILE TRAFFIC SIGNAL SYSTEM |  | 4101030 | 1 | NMDOT |
| 450 | 702810 | 1 | LS | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION |  | 4101030 | 1 | NMDOT |
| 460 | 704000 | 300000 | L.F. | RETROREFLECTORIZED PAINTED MARKINGS 4" |  | 4101030 | 1 | NMDOT |
| 470 | 704099 | 3400 | L.F. | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" |  | 4101030 | 1 | NMDOT |
| 480 | 704875 | 4230 | EACH | TEMPORARY REFLECTIVE RAISED PAVEMENT MARKER, TYPE TD | 4101030 | 1 | NMDOT |
| 490 | 720060 | 4 | EACH | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES |  | 4101030 | 1 | NMDOT |
| 500 | 720110 | 4 | EACH | REMOVE/RESET IMPACT ATTENUATOR UNIT |  | 4101030 | 1 | NMDOT |
| 510 | 721000 | 2000 | L.F. | REMOVAL OF PAVEMENT MARKING |  | 4101030 | 1 | NMDOT |
| 520 | 801000 | 1 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  | 4101030 | 1 | NMDOT |
| 530 | 802000 | 1 | LS | POST CONSTRUCTION PLANS | 5000 | 4101030 | 1 | NMDOT |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Line | Item | Quantity | Unit | Description | Price | Proposal | Call Order | Agency ID |
| 10 | 403701 | 5254 | TON | OPEN GRADED FRICTION COURSE COMPLETE |  | 2104690 | 2 | NMDOT |
| 20 | 407000 | 179 | TON | ASPHALT MATERIAL FOR TACK COAT |  | 2104690 | 2 | NMDOT |
| 30 | 407001 | 11 | TON | FOG SEAL |  | 2104690 | 2 | NMDOT |
| 40 | 414000 | 1051872 | SYIN | COLD MILLING (ASPHALT) |  | 2104690 | 2 | NMDOT |
| 50 | 423283 | 55358 | TON | HMA SP-IV COMPLETE |  | 2104690 | 2 | NMDOT |
| 60 | 618000 | 1 | LS | TRAFFIC CONTROL MANAGEMENT |  | 2104690 | 2 | NMDOT |
| 70 | 621000 | 1 | LS | MOBILIZATION |  | 2104690 | 2 | NMDOT |
| 80 | 631000 | 75476 | L.F. | RUMBLE STRIPS |  | 2104690 | 2 | NMDOT |
| 90 | 702000 | 1512 | S.F. | CONSTRUCTION SIGNING |  | 2104690 | 2 | NMDOT |
| 100 | 702100 | 948 | L.F. | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING |  | 2104690 | 2 | NMDOT |
| 110 | 702101 | 48 | EACH | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING |  | 2104690 | 2 | NMDOT |
| 120 | 702110 | 54 | EACH | PORTABLE SIGN SUPPORT |  | 2104690 | 2 | NMDOT |
| 130 | 702525 | 410 | EACH | CHANNELIZATION DEVICES TYPE DRUM |  | 2104690 | 2 | NMDOT |
| 140 | 702600 | 2 | EACH | SEQUENTIAL ARROW DISPLAY |  | 2104690 | 2 | NMDOT |
| 150 | 702610 | 2 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  | 2104690 | 2 | NMDOT |
| 160 | 702613 | 2 | EACH | SPEED DETECTOR RADAR TRAILER |  | 2104690 | 2 | NMDOT |
| 170 | 704000 | 240381 | L.F. | RETROREFLECTORIZED PAINTED MARKINGS 4" |  | 2104690 | 2 | NMDOT |
| 180 | 704099 | 120241 | L.F. | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" |  | 2104690 | 2 | NMDOT |
| 190 | 750000 | 1 | LS | INTELLIGENT TRANSPORTATION SYSTEM |  | 2104690 | 2 | NMDOT |
| 200 | 801000 | 1 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  | 2104690 | 2 | NMDOT |
| 210 | 802000 | 1 | LS | POST CONSTRUCTION PLANS | 5000 | 2104690 | 2 | NMDOT |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Line | Item | Quantity | Unit | Description | Price | Proposal | Call Order | Agency ID |
| 10 | 210002 | 780 | C.Y. | MAJOR STRUCTURE EXCAVATION |  | 2104910 | 3 | NMDOT |
| 20 | 210003 | 1580 | C.Y. | MAJOR STRUCTURE BACKFILL |  | 2104910 | 3 | NMDOT |
| 30 | 511030 | 190 | C.Y. | STRUCTURAL CONCRETE, CLASS AA |  | 2104910 | 3 | NMDOT |
| 40 | 511802 | 80 | L.F. | PRECAST CONCRETE BOX CULVERT, 7.5'-12.4' |  | 2104910 | 3 | NMDOT |
| 50 | 540060 | 19950 | LB | REINFORCING BARS GRADE 60 |  | 2104910 | 3 | NMDOT |
| 60 | 564000 | 42 | L.F. | PREFORMED CLOSED CELL FOAM BRIDGE JOINT SEALS |  | 2104910 | 3 | NMDOT |
| 70 | 601000 | 1 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  | 2104910 | 3 | NMDOT |
| 80 | 604300 | 3310 | S.Y. | GEOGRID REINFORCEMENT |  | 2104910 | 3 | NMDOT |
| 90 | 201000 | 1 | LS | CLEARING AND GRUBBING |  | 2104910 | 3 | NMDOT |
| 100 | 203000 | 3300 | C.Y. | UNCLASSIFIED EXCAVATION |  | 2104910 | 3 | NMDOT |
| 110 | 203100 | 1500 | C.Y. | BORROW |  | 2104910 | 3 | NMDOT |
| 120 | 203211 | 1300 | S.Y. | UNSTABLE SUBGRADE STABILIZATION |  | 2104910 | 3 | NMDOT |
| 130 | 207000 | 8890 | S.Y. | SUBGRADE PREPARATION |  | 2104910 | 3 | NMDOT |
| 140 | 210010 | 1 | LS | TEMPORARY RETAINING WALL/SHORING |  | 2104910 | 3 | NMDOT |
| 150 | 303000 | 2290 | TON | BASE COURSE |  | 2104910 | 3 | NMDOT |
| 160 | 303160 | 690 | S.Y. | BASE COURSE 6" |  | 2104910 | 3 | NMDOT |
| 170 | 403701 | 170 | TON | OPEN GRADED FRICTION COURSE COMPLETE |  | 2104910 | 3 | NMDOT |
| 180 | 405000 | 3300 | S.Y. | DETOUR PAVEMENT CONSTRUCTION |  | 2104910 | 3 | NMDOT |
| 190 | 407000 | 5 | TON | ASPHALT MATERIAL FOR TACK COAT |  | 2104910 | 3 | NMDOT |
| 200 | 408100 | 14 | TON | PRIME COAT MATERIAL |  | 2104910 | 3 | NMDOT |
| 210 | 416104 | 2210 | TON | MINOR PAVING TYPE I, HMA SP-IV |  | 2104910 | 3 | NMDOT |
| 220 | 416207 | 120 | S.Y. | MINOR PAVING TYPE II, HMA SP-IV |  | 2104910 | 3 | NMDOT |
| 230 | 515000 | 33 | C.Y. | REINF.CONCRETE FOR MINOR STRUCTURES |  | 2104910 | 3 | NMDOT |
| 240 | 540060 | 2150 | LB | REINFORCING BARS GRADE 60 |  | 2104910 | 3 | NMDOT |
| 250 | 570182 | 56 | L.F. | 83"SX57"R (NOMINAL) CULVERT PIPE ARCH |  | 2104910 | 3 | NMDOT |
| 260 | 601000 | 1 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  | 2104910 | 3 | NMDOT |
| 270 | 601110 | 4070 | S.Y. | REMOVAL OF SURFACING |  | 2104910 | 3 | NMDOT |
| 280 | 602060 | 400 | S.Y. | RIPRAP CLASS G |  | 2104910 | 3 | NMDOT |
| 290 | 603100 | 1 | ACRE | TEMPORARY SOIL STABILANT |  | 2104910 | 3 | NMDOT |
| 300 | 603262 | 1000 | L.F. | COMPOSTED MULCH SOCKS |  | 2104910 | 3 | NMDOT |
| 310 | 603281 | 1 | LS | SWPPP PLAN PREPARATION AND MAINTENANCE |  | 2104910 | 3 | NMDOT |
| 320 | 606001 | 300 | L.F. | SINGLE FACE W-BEAM GUARDRAIL |  | 2104910 | 3 | NMDOT |
| 330 | 606051 | 4 | EACH | END TREATMENT TL-3 END TERMINAL |  | 2104910 | 3 | NMDOT |
| 340 | 606062 | 4 | EACH | TRANSITION METAL BARRIER TO RIGID BARRIER |  | 2104910 | 3 | NMDOT |
| 350 | 606542 | 96 | L.F. | CONCRETE WALL BARRIER 42" |  | 2104910 | 3 | NMDOT |
| 360 | 606598 | 1140 | L.F. | TCWB RETAINED BY THE CONTRACTOR |  | 2104910 | 3 | NMDOT |
| 370 | 606599 | 920 | L.F. | RESETTING OF TCWB |  | 2104910 | 3 | NMDOT |
| 380 | 607004 | 1060 | L.F. | BARBED WIRE FENCE 4' |  | 2104910 | 3 | NMDOT |
| 390 | 607015 | 11 | EACH | BRACES/CORNER POSTS |  | 2104910 | 3 | NMDOT |
| 400 | 607251 | 2 | EACH | REMOVE AND RESET GATE |  | 2104910 | 3 | NMDOT |
| 410 | 610000 | 24 | L.F. | CATTLE GUARD |  | 2104910 | 3 | NMDOT |
| 420 | 618000 | 1 | LS | TRAFFIC CONTROL MANAGEMENT |  | 2104910 | 3 | NMDOT |
| 430 | 618011 | 1 | LS | PUBLIC AWARENESS | 5000 | 2104910 | 3 | NMDOT |
| 440 | 621000 | 1 | LS | MOBILIZATION |  | 2104910 | 3 | NMDOT |
| 450 | 632000 | 1 | ACRE | CLASS A SEEDING |  | 2104910 | 3 | NMDOT |
| 460 | 663049 | 1 | LS | PRECONSTRUCTION UTILITY SURVEY |  | 2104910 | 3 | NMDOT |
| 470 | 667110 | 2 | EACH | MAIL BOX INSTALLATION-SINGLE |  | 2104910 | 3 | NMDOT |
| 480 | 701000 | 40 | S.F. | PANEL SIGNS |  | 2104910 | 3 | NMDOT |
| 490 | 701100 | 110 | L.F. | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS |  | 2104910 | 3 | NMDOT |
| 500 | 702000 | 360 | S.F. | CONSTRUCTION SIGNING |  | 2104910 | 3 | NMDOT |
| 510 | 702100 | 450 | L.F. | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING |  | 2104910 | 3 | NMDOT |
| 520 | 702101 | 8 | EACH | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING | 2104910 | 3 | NMDOT |
| 530 | 702238 | 4 | EACH | BARRICADE, TYPE III-8' |  | 2104910 | 3 | NMDOT |
| 540 | 702320 | 58 | EACH | VERTICAL PANEL, TYPE BACK TO BACK |  | 2104910 | 3 | NMDOT |
| 550 | 702525 | 59 | EACH | CHANNELIZATION DEVICES TYPE DRUM |  | 2104910 | 3 | NMDOT |
| 560 | 702610 | 2 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  | 2104910 | 3 | NMDOT |
| 570 | 702710 | 1 | EACH | MOBILE TRAFFIC SIGNAL SYSTEM |  | 2104910 | 3 | NMDOT |
| 580 | 704000 | 14080 | L.F. | RETROREFLECTORIZED PAINTED MARKINGS 4" |  | 2104910 | 3 | NMDOT |
| 590 | 704099 | 3800 | L.F. | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" |  | 2104910 | 3 | NMDOT |
| 600 | 720060 | 4 | EACH | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES |  | 2104910 | 3 | NMDOT |
| 610 | 720110 | 6 | EACH | REMOVE/RESET IMPACT ATTENUATOR UNIT |  | 2104910 | 3 | NMDOT |
| 620 | 721000 | 6000 | L.F. | REMOVAL OF PAVEMENT MARKING |  | 2104910 | 3 | NMDOT |
| 630 | 801000 | 1 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  | 2104910 | 3 | NMDOT |
| 640 | 802000 | 1 | LS | POST CONSTRUCTION PLANS | 5000 | 2104910 | 3 | NMDOT |