|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Line | Item | Quantity | Unit | Description | Price | Proposal |
| 10 | 203301 | 45 | C.Y. | ROCK EXCAVATION |  | 5101174 |
| 20 | 210002 | 1150 | C.Y. | MAJOR STRUCTURE EXCAVATION |  | 5101174 |
| 30 | 210003 | 520 | C.Y. | MAJOR STRUCTURE BACKFILL |  | 5101174 |
| 40 | 210010 | 1 | LS | TEMPORARY RETAINING WALL/SHORING |  | 5101174 |
| 50 | 502042 | 366 | L.F. | DRILLED SHAFT FOUNDATION 42" DIAMETER |  | 5101174 |
| 60 | 502054 | 243 | L.F. | DRILLED SHAFT FOUNDATION 54" DIAMETER |  | 5101174 |
| 70 | 502160 | 90 | L.F. | PERMANENT CASING 60" DIAMETER |  | 5101174 |
| 80 | 502600 | 94 | L.F. | OBSTRUCTION REMOVAL |  | 5101174 |
| 90 | 505001 | 18 | EACH | CROSSHOLE SONIC LOGGING DEPARTMENT TESTING |  | 5101174 |
| 100 | 505010 | 18 | EACH | LOW STRAIN INTEGRITY DEPARTMENT TESTING |  | 5101174 |
| 110 | 511000 | 252 | C.Y. | STRUCTURAL CONCRETE, CLASS A |  | 5101174 |
| 120 | 511070 | 981 | C.Y. | STRUCTURAL CONCRETE, CLASS HPD |  | 5101174 |
| 130 | 514042 | 1090 | L.F. | CONCRETE BARRIER RAILINGS 42" |  | 5101174 |
| 140 | 518063 | 2295 | L.F. | PRESTRESSED CONCRETE BRIDGE MEMBER TYPE 63 |  | 5101174 |
| 150 | 535100 | 2448 | S.Y. | CONCRETE SURFACE TREATMENT |  | 5101174 |
| 160 | 536001 | 2448 | S.Y. | EPOXY URETHANE POLYMER CONCRETE BRIDGE DECK OVERLAY |  | 5101174 |
| 170 | 540060 | 103800 | LB | REINFORCING BARS GRADE 60 |  | 5101174 |
| 180 | 540061 | 208800 | LB | GALVANIZED BARS GRADE 60 |  | 5101174 |
| 190 | 540170 | 170 | EACH | MECHANICAL COUPLERS |  | 5101174 |
| 200 | 541000 | 26472 | LB | STRUCTURAL STEEL FOR CONCRETE BRIDGES |  | 5101174 |
| 210 | 560000 | 40 | EACH | ELASTOMERIC BEARING PADS |  | 5101174 |
| 220 | 562000 | 180 | L.F. | BRIDGE JOINT STRIP SEAL |  | 5101174 |
| 230 | 563099 | 172 | L.F. | POLYMER BRIDGE JOINT SEALS |  | 5101174 |
| 240 | 601000 | 1 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  | 5101174 |
| 250 | 604002 | 814 | S.Y. | GEOTEXTILE CLASS 2 |  | 5101174 |
| 260 | 604300 | 5210 | S.Y. | GEOGRID REINFORCEMENT |  | 5101174 |
| 270 | 107000 | 1 | LS | ENVIRONMENTAL COMMITMENTS |  | 5101174 |
| 280 | 201000 | 1 | LS | CLEARING AND GRUBBING |  | 5101174 |
| 290 | 203000 | 63800 | C.Y. | UNCLASSIFIED EXCAVATION |  | 5101174 |
| 300 | 203100 | 2000 | C.Y. | BORROW |  | 5101174 |
| 310 | 203200 | 3000 | C.Y. | UNSUITABLE MATERIAL EXCAVATION |  | 5101174 |
| 320 | 203211 | 3060 | S.Y. | UNSTABLE SUBGRADE STABILIZATION |  | 5101174 |
| 330 | 203301 | 3060 | C.Y. | ROCK EXCAVATION |  | 5101174 |
| 340 | 207000 | 22800 | S.Y. | SUBGRADE PREPARATION |  | 5101174 |
| 350 | 303000 | 14500 | TON | BASE COURSE |  | 5101174 |
| 360 | 303140 | 1800 | S.Y. | BASE COURSE 4" |  | 5101174 |
| 370 | 303160 | 2500 | S.Y. | BASE COURSE 6" |  | 5101174 |
| 380 | 306102 | 37900 | S.Y. | LIME TREATED SUBGRADE 12" |  | 5101174 |
| 390 | 403701 | 1060 | TON | OPEN GRADED FRICTION COURSE COMPLETE |  | 5101174 |
| 400 | 405000 | 12050 | S.Y. | DETOUR PAVEMENT CONSTRUCTION |  | 5101174 |
| 410 | 407000 | 26 | TON | ASPHALT MATERIAL FOR TACK COAT |  | 5101174 |
| 420 | 408100 | 91 | TON | PRIME COAT MATERIAL |  | 5101174 |
| 430 | 416207 | 2050 | S.Y. | MINOR PAVING TYPE II, HMA SP-IV |  | 5101174 |
| 440 | 417000 | 320 | S.Y. | MISCELLANEOUS PAVING |  | 5101174 |
| 450 | 423283 | 15100 | TON | HMA SP-IV COMPLETE |  | 5101174 |
| 460 | 502030 | 16.5 | L.F. | DRILLED SHAFT FOUNDATION 30" DIAMETER |  | 5101174 |
| 470 | 511000 | 90 | C.Y. | STRUCTURAL CONCRETE, CLASS A |  | 5101174 |
| 480 | 515000 | 50 | C.Y. | REINF.CONCRETE FOR MINOR STRUCTURES |  | 5101174 |
| 490 | 540060 | 530 | LB | REINFORCING BARS GRADE 60 |  | 5101174 |
| 500 | 541200 | 3100 | LB | STRUCTURAL STEEL FOR MISCELLANEOUS STRUCTURES |  | 5101174 |
| 510 | 570024 | 770 | L.F. | 24" CULVERT PIPE |  | 5101174 |
| 520 | 570025 | 4 | EACH | 24" CULVERT PIPE END SECTION |  | 5101174 |
| 530 | 570026 | 310 | L.F. | 24" CULVERT PIPE - SLIP LINING |  | 5101174 |
| 540 | 570030 | 160 | L.F. | 30" CULVERT PIPE |  | 5101174 |
| 550 | 570036 | 210 | L.F. | 36" CULVERT PIPE |  | 5101174 |
| 560 | 570037 | 2 | EACH | 36" CULVERT PIPE END SECTION |  | 5101174 |
| 570 | 570060 | 320 | L.F. | 60" CULVERT PIPE |  | 5101174 |
| 580 | 570156 | 140 | L.F. | 28"SX20"R (NOMINAL) CULVERT PIPE ARCH |  | 5101174 |
| 590 | 570157 | 2 | EACH | 28"SX20"R (NOMINAL) CULVERT PIPE ARCH END SECTION |  | 5101174 |
| 600 | 601000 | 1 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  | 5101174 |
| 610 | 601110 | 42000 | S.Y. | REMOVAL OF SURFACING |  | 5101174 |
| 620 | 602000 | 3330 | C.Y. | RIPRAP CLASS A |  | 5101174 |
| 630 | 602005 | 8 | C.Y. | RIPRAP CLASS A (NON-ENCLOSED) |  | 5101174 |
| 640 | 602010 | 10 | C.Y. | RIPRAP CLASS B |  | 5101174 |
| 650 | 602060 | 4530 | S.Y. | RIPRAP CLASS G |  | 5101174 |
| 660 | 602200 | 20 | C.Y. | GABIONS |  | 5101174 |
| 670 | 603100 | 13 | ACRE | TEMPORARY SOIL STABILANT |  | 5101174 |
| 680 | 603221 | 900 | L.F. | ROCK CHECK DAM |  | 5101174 |
| 690 | 603262 | 700 | L.F. | COMPOSTED MULCH SOCKS |  | 5101174 |
| 700 | 603281 | 1 | LS | SWPPP PLAN PREPARATION AND MAINTENANCE |  | 5101174 |
| 710 | 606001 | 2875 | L.F. | SINGLE FACE W-BEAM GUARDRAIL |  | 5101174 |
| 720 | 606051 | 10 | EACH | END TREATMENT TL-3 END TERMINAL |  | 5101174 |
| 730 | 606055 | 2 | EACH | END TREATMENT DRIVEWAY END ANCHOR |  | 5101174 |
| 740 | 606061 | 87.5 | L.F. | DRAINAGE STRUCTURE PROTECTION SYSTEM |  | 5101174 |
| 750 | 606062 | 8 | EACH | TRANSITION METAL BARRIER TO RIGID BARRIER |  | 5101174 |
| 760 | 606710 | 2720 | L.F. | TCWB RETAINED BY THE CONTRACTOR (20') |  | 5101174 |
| 770 | 606719 | 840 | L.F. | RESETTING OF TCWB (20') |  | 5101174 |
| 780 | 607014 | 18870 | L.F. | WOVEN WIRE FENCE 4' |  | 5101174 |
| 790 | 607015 | 120 | EACH | BRACES/CORNER POSTS |  | 5101174 |
| 800 | 607316 | 6 | EACH | STANDARD GATE, 16' |  | 5101174 |
| 810 | 607320 | 3 | EACH | STANDARD GATE, 20' |  | 5101174 |
| 820 | 613000 | 1 | LS | CLEANING CULVERTS AND DRAINAGE STRUCTURES |  | 5101174 |
| 830 | 618000 | 1 | LS | TRAFFIC CONTROL MANAGEMENT |  | 5101174 |
| 840 | 618011 | 1 | LS | PUBLIC AWARENESS | 15000 | 5101174 |
| 850 | 621000 | 1 | LS | MOBILIZATION |  | 5101174 |
| 860 | 622002 | 1 | EACH | FIELD LABORATORY, TYPE II |  | 5101174 |
| 870 | 622100 | 1 | EACH | SUPPLEMENTAL FIELD LABORATORY |  | 5101174 |
| 880 | 622110 | 1 | EACH | SUPPLEMENTAL HOT-MIX ASPHALT FIELD LABORATORY |  | 5101174 |
| 890 | 622200 | 1 | EACH | FIELD OFFICE |  | 5101174 |
| 900 | 631000 | 21700 | L.F. | RUMBLE STRIPS |  | 5101174 |
| 910 | 632000 | 10 | ACRE | CLASS A SEEDING |  | 5101174 |
| 920 | 632010 | 2 | ACRE | CLASS B SEEDING |  | 5101174 |
| 930 | 632020 | 2 | ACRE | CLASS C SEEDING |  | 5101174 |
| 940 | 701000 | 430 | S.F. | PANEL SIGNS |  | 5101174 |
| 950 | 701100 | 880 | L.F. | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS |  | 5101174 |
| 960 | 702000 | 200 | S.F. | CONSTRUCTION SIGNING |  | 5101174 |
| 970 | 702100 | 100 | L.F. | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING |  | 5101174 |
| 980 | 702101 | 12 | EACH | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING | | 5101174 |
| 990 | 702610 | 2 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  | 5101174 |
| 1000 | 702612 | 5 | EACH | PORTABLE FLOODLIGHT SYSTEM |  | 5101174 |
| 1010 | 702710 | 2 | EACH | MOBILE TRAFFIC SIGNAL SYSTEM |  | 5101174 |
| 1020 | 702810 | 1 | LS | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION |  | 5101174 |
| 1030 | 703002 | 28 | EACH | OBJECT MARKER TYPE 2 |  | 5101174 |
| 1040 | 703003 | 8 | EACH | OBJECT MARKER TYPE 3 |  | 5101174 |
| 1050 | 704000 | 120900 | L.F. | RETROREFLECTORIZED PAINTED MARKINGS 4" |  | 5101174 |
| 1060 | 704003 | 1620 | L.F. | RETROREFLECTORIZED PAINTED MARKINGS 8" |  | 5101174 |
| 1070 | 704005 | 330 | L.F. | RETROREFLECTORIZED PAINTED MARKINGS 24" |  | 5101174 |
| 1080 | 704099 | 198084 | L.F. | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" |  | 5101174 |
| 1090 | 704718 | 3 | EACH | HOT THERMOPLASTIC PAVEMENT MARKING LEFT ARROW |  | 5101174 |
| 1100 | 704720 | 2 | EACH | HOT THERMOPLASTIC PAVEMENT MARKING WORD (ONLY) |  | 5101174 |
| 1110 | 704868 | 36 | EACH | PLOWABLE REFLECTIVE RAISED PAVEMENT MARKER TYPE PD |  | 5101174 |
| 1120 | 705000 | 1 | ALOW | SIGNAL/LIGHTING SYSTEM START-UP COSTS | 5000 | 5101174 |
| 1130 | 706010 | 1 | EACH | SERVICE POLE (LIGHTING) |  | 5101174 |
| 1140 | 706110 | 1 | EACH | SERVICE RISER (LIGHTING) |  | 5101174 |
| 1150 | 706350 | 1 | LS | POWER SERVICE INSTALLATION | 20000 | 5101174 |
| 1160 | 706420 | 1 | EACH | LIGHTING CONTROL CABINET-TWO CIRCUIT |  | 5101174 |
| 1170 | 707540 | 2 | EACH | TYPE V STANDARD, 40' |  | 5101174 |
| 1180 | 709020 | 500 | L.F. | RIGID ELECTRICAL CONDUIT 2" (DIA.) |  | 5101174 |
| 1190 | 709030 | 610 | L.F. | RIGID ELECTRICAL CONDUIT 3" (DIA.) |  | 5101174 |
| 1200 | 710000 | 3 | EACH | ELECTRICAL PULL BOX (STANDARD) |  | 5101174 |
| 1210 | 711102 | 1100 | L.F. | SINGLE CONDUCTOR 2 |  | 5101174 |
| 1220 | 711106 | 550 | L.F. | SINGLE CONDUCTOR 6 |  | 5101174 |
| 1230 | 711240 | 170 | L.F. | SINGLE CONDUCTOR 4/0 |  | 5101174 |
| 1240 | 716701 | 2 | EACH | LED ROADWAY LUMINAIRE |  | 5101174 |
| 1250 | 720060 | 10 | EACH | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES |  | 5101174 |
| 1260 | 720110 | 6 | EACH | REMOVE/RESET IMPACT ATTENUATOR UNIT |  | 5101174 |
| 1270 | 721000 | 71038 | L.F. | REMOVAL OF PAVEMENT MARKING |  | 5101174 |
| 1280 | 750000 | 1 | LS | INTELLIGENT TRANSPORTATION SYSTEM |  | 5101174 |
| 1290 | 750032 | 10200 | L.F. | MULTI-DUCT CONDUIT 2" (8-WAY) |  | 5101174 |
| 1300 | 750060 | 7 | EACH | ITS PULLBOX (33"X24"X24") |  | 5101174 |
| 1310 | 750080 | 3 | EACH | ITS MANHOLE (48"X48"X48") |  | 5101174 |
| 1320 | 801000 | 1 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  | 5101174 |
| 1330 | 802000 | 1 | LS | POST CONSTRUCTION PLANS | 50000 | 5101174 |
| 1340 | 802010 | 1 | LS | CAMP DATA COLLECTION |  | 5101174 |
| 1350 | 803000 | 1 | LS | SCHEDULE SOFTWARE |  | 5101174 |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Line | Item | Quantity | Unit | Description | Price | Proposal |
| 10 | 403715 | 7357 | TON | RUBBERIZED OPEN-GRADED FRICTION COURSE COMPLETE |  | 1101900 |
| 20 | 407000 | 332 | TON | ASPHALT MATERIAL FOR TACK COAT |  | 1101900 |
| 30 | 414000 | 2316950 | SYIN | COLD MILLING (ASPHALT) |  | 1101900 |
| 40 | 414010 | 114500 | SYIN | COLD MILLING (CONCRETE) |  | 1101900 |
| 50 | 423283 | 114966 | TON | HMA SP-IV COMPLETE |  | 1101900 |
| 60 | 601000 | 1 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  | 1101900 |
| 70 | 606001 | 14062.5 | L.F. | SINGLE FACE W-BEAM GUARDRAIL |  | 1101900 |
| 80 | 606051 | 50 | EACH | END TREATMENT TL-3 END TERMINAL |  | 1101900 |
| 90 | 606053 | 12 | EACH | END TREATMENT W-BEAM END ANCHOR |  | 1101900 |
| 100 | 606062 | 50 | EACH | TRANSITION METAL BARRIER TO RIGID BARRIER |  | 1101900 |
| 110 | 606542 | 6013 | L.F. | CONCRETE WALL BARRIER 42" |  | 1101900 |
| 120 | 618000 | 1 | LS | TRAFFIC CONTROL MANAGEMENT |  | 1101900 |
| 130 | 621000 | 1 | LS | MOBILIZATION |  | 1101900 |
| 140 | 622100 | 1 | EACH | SUPPLEMENTAL FIELD LABORATORY |  | 1101900 |
| 150 | 631000 | 192000 | L.F. | RUMBLE STRIPS |  | 1101900 |
| 160 | 701000 | 479 | S.F. | PANEL SIGNS |  | 1101900 |
| 170 | 701010 | 60 | S.F. | EXTRUDED PANEL SIGNS |  | 1101900 |
| 180 | 701100 | 1070 | L.F. | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS |  | 1101900 |
| 190 | 701109 | 50 | L.F. | STEEL I-BEAM POST TYPE W6X9 |  | 1101900 |
| 200 | 701209 | 4 | EACH | BREAKAWAY BASE SYSTEM FOR STEEL I BEAM POST W6X9 |  | 1101900 |
| 210 | 702000 | 1340 | S.F. | CONSTRUCTION SIGNING |  | 1101900 |
| 220 | 702100 | 1397 | L.F. | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING |  | 1101900 |
| 230 | 702101 | 12 | EACH | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING |  | 1101900 |
| 240 | 702110 | 34 | EACH | PORTABLE SIGN SUPPORT |  | 1101900 |
| 250 | 702238 | 4 | EACH | BARRICADE, TYPE III-8' |  | 1101900 |
| 260 | 702525 | 330 | EACH | CHANNELIZATION DEVICES TYPE DRUM |  | 1101900 |
| 270 | 702600 | 2 | EACH | SEQUENTIAL ARROW DISPLAY |  | 1101900 |
| 280 | 702610 | 3 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  | 1101900 |
| 290 | 702613 | 2 | EACH | SPEED DETECTOR RADAR TRAILER |  | 1101900 |
| 300 | 702850 | 1 | ALOW | LAW ENFORCEMENT IN CONSTRUCTION ZONE | 30000 | 1101900 |
| 310 | 704099 | 218336 | L.F. | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" |  | 1101900 |
| 320 | 704760 | 3100 | L.F. | DOUBLE DROP HOT THERMOPLASTIC PAVEMENT MARKINGS 4" |  | 1101900 |
| 330 | 704761 | 218400 | L.F. | DOUBLE DROP HOT THERMOPLASTIC PAVEMENT MARKINGS 6" |  | 1101900 |
| 340 | 704763 | 2400 | L.F. | DOUBLE DROP HOT THERMOPLASTIC PAVEMENT MARKINGS 12" |  | 1101900 |
| 350 | 704869 | 50 | EACH | PLOWABLE REFLECTIVE RAISED PAVEMENT MARKER TYPE PG |  | 1101900 |
| 360 | 704871 | 4855 | EACH | PLOWABLE REFLECTIVE RAISED PAVEMENT MARKER TYPE PJ |  | 1101900 |
| 370 | 704872 | 2430 | EACH | PLOWABLE REFLECTIVE RAISED PAVEMENT MARKER TYPE PC |  | 1101900 |
| 380 | 801000 | 1 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  | 1101900 |
| 390 | 802000 | 1 | LS | POST CONSTRUCTION PLANS | 5000 | 1101900 |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Line | Item | Quantity | Unit | Description | Price | Proposal |
| 10 | 301000 | 205150 | S.Y. | FULL DEPTH RECLAMATION |  | 2104830 |
| 20 | 301014 | 2220 | TON | ASPHALT BINDER |  | 2104830 |
| 30 | 301015 | 950 | TON | MINERAL FILLER |  | 2104830 |
| 40 | 403701 | 7140 | TON | OPEN GRADED FRICTION COURSE COMPLETE |  | 2104830 |
| 50 | 407000 | 224 | TON | ASPHALT MATERIAL FOR TACK COAT |  | 2104830 |
| 60 | 414000 | 1117700 | SYIN | COLD MILLING (ASPHALT) |  | 2104830 |
| 70 | 423283 | 54840 | TON | HMA SP-IV COMPLETE |  | 2104830 |
| 80 | 613000 | 1 | LS | CLEANING CULVERTS AND DRAINAGE STRUCTURES |  | 2104830 |
| 90 | 618000 | 1 | LS | TRAFFIC CONTROL MANAGEMENT |  | 2104830 |
| 100 | 621000 | 1 | LS | MOBILIZATION |  | 2104830 |
| 110 | 631000 | 137850 | L.F. | RUMBLE STRIPS |  | 2104830 |
| 120 | 702000 | 1136 | S.F. | CONSTRUCTION SIGNING |  | 2104830 |
| 130 | 702100 | 754 | L.F. | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING |  | 2104830 |
| 140 | 702101 | 48 | EACH | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING |  | 2104830 |
| 150 | 702110 | 22 | EACH | PORTABLE SIGN SUPPORT |  | 2104830 |
| 160 | 702525 | 269 | EACH | CHANNELIZATION DEVICES TYPE DRUM |  | 2104830 |
| 170 | 702600 | 1 | EACH | SEQUENTIAL ARROW DISPLAY |  | 2104830 |
| 180 | 702610 | 2 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  | 2104830 |
| 190 | 704099 | 216700 | L.F. | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" |  | 2104830 |
| 200 | 704700 | 162518 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKINGS 4" |  | 2104830 |
| 210 | 801000 | 1 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  | 2104830 |
| 220 | 802000 | 1 | LS | POST CONSTRUCTION PLANS | 5000 | 2104830 |
| 230 | 802010 | 1 | LS | CAMP DATA COLLECTION |  | 2104830 |
|  |  |  |  |  |  |  |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Line | Item | Quantity | Unit | Description | Price | Proposal |
| 10 | 201000 | 1 | LS | CLEARING AND GRUBBING |  | S100682 |
| 20 | 203000 | 7400 | C.Y. | UNCLASSIFIED EXCAVATION |  | S100682 |
| 30 | 203211 | 1270 | S.Y. | UNSTABLE SUBGRADE STABILIZATION |  | S100682 |
| 40 | 207000 | 8470 | S.Y. | SUBGRADE PREPARATION |  | S100682 |
| 50 | 210002 | 22760 | C.Y. | MAJOR STRUCTURE EXCAVATION |  | S100682 |
| 60 | 210003 | 14510 | C.Y. | MAJOR STRUCTURE BACKFILL |  | S100682 |
| 70 | 303140 | 8470 | S.Y. | BASE COURSE 4" |  | S100682 |
| 80 | 407000 | 3 | TON | ASPHALT MATERIAL FOR TACK COAT |  | S100682 |
| 90 | 408100 | 16 | TON | PRIME COAT MATERIAL |  | S100682 |
| 100 | 416113 | 1190 | TON | MINOR PAVING TYPE I, WMA SP-III |  | S100682 |
| 110 | 450060 | 180 | S.Y. | CONCRETE PAVEMENT-6" |  | S100682 |
| 120 | 511000 | 90 | C.Y. | STRUCTURAL CONCRETE, CLASS A |  | S100682 |
| 130 | 540060 | 7210 | LB | REINFORCING BARS GRADE 60 |  | S100682 |
| 140 | 570018 | 20 | L.F. | 18" CULVERT PIPE |  | S100682 |
| 150 | 570019 | 2 | EACH | 18" CULVERT PIPE END SECTION |  | S100682 |
| 160 | 570425 | 200 | L.F. | 18" STORM DRAIN CULVERT PIPE |  | S100682 |
| 170 | 570429 | 1 | EACH | 18" STORM DRAIN CULVERT PIPE END SECTION |  | S100682 |
| 180 | 570437 | 860 | L.F. | 24" STORM DRAIN CULVERT PIPE |  | S100682 |
| 190 | 570461 | 240 | L.F. | 36" STORM DRAIN CULVERT PIPE |  | S100682 |
| 200 | 601000 | 1 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  | S100682 |
| 210 | 601110 | 18300 | S.Y. | REMOVAL OF SURFACING |  | S100682 |
| 220 | 602005 | 30 | C.Y. | RIPRAP CLASS A (NON-ENCLOSED) |  | S100682 |
| 230 | 603281 | 1 | LS | SWPPP PLAN PREPARATION AND MAINTENANCE |  | S100682 |
| 240 | 605300 | 1 | LS | UNDERGROUND DETENTION AND INFILTRATION SYSTEM |  | S100682 |
| 250 | 607220 | 710 | L.F. | REMOVE AND REBUILD CHAIN LINK FENCE |  | S100682 |
| 260 | 607250 | 3 | EACH | REMOVE AND RESET CHAIN LINK GATE |  | S100682 |
| 270 | 607251 | 2 | EACH | REMOVE AND RESET GATE |  | S100682 |
| 280 | 608004 | 1470 | S.Y. | CONCRETE SIDEWALK 4" |  | S100682 |
| 290 | 608020 | 10 | S.Y. | SIDEWALK CULVERT (SINGLE) |  | S100682 |
| 300 | 608204 | 35 | S.Y. | CONCRETE MEDIAN PAVEMENT 4" |  | S100682 |
| 310 | 609006 | 1000 | L.F. | CONCRETE CURB 6" |  | S100682 |
| 320 | 609424 | 3400 | L.F. | CONCRETE VERTICAL CURB AND GUTTER TYPE B 6" X 24" |  | S100682 |
| 330 | 609648 | 600 | L.F. | CONCRETE VALLEY GUTTER 6" X 48" |  | S100682 |
| 340 | 617000 | 1 | LS | VIBRATION MONITORING |  | S100682 |
| 350 | 617003 | 1 | LS | VIDEO RECORDING |  | S100682 |
| 360 | 618000 | 1 | LS | TRAFFIC CONTROL MANAGEMENT |  | S100682 |
| 370 | 621000 | 1 | LS | MOBILIZATION |  | S100682 |
| 380 | 623104 | 1 | EACH | MEDIAN DROP INLET 5'X5' (URBAN) H=0'0" TO 3'0" |  | S100682 |
| 390 | 623105 | 1 | EACH | MEDIAN DROP INLET 5'X5' (URBAN) H=3'1" TO 6'0" |  | S100682 |
| 400 | 623108 | 1 | EACH | MEDIAN DROP INLET 5'X5' (URBAN) H=12'1" TO 15'0" |  | S100682 |
| 410 | 623501 | 1 | EACH | TRANSVERSE DROP INLET TYPE I, 0' TO 8' |  | S100682 |
| 420 | 623600 | 1 | EACH | JUNCTION BOX |  | S100682 |
| 430 | 623900 | 1 | LS | DROP INLET SPECIAL DESIGN COMPLETE |  | S100682 |
| 440 | 662022 | 1 | EACH | MANHOLE TYPE C-6' DIAMETER OVER 6' TO 10' DEPTH |  | S100682 |
| 450 | 662024 | 3 | EACH | MANHOLE TYPE C-6' DIAMETER OVER 10' TO 14' DEPTH |  | S100682 |
| 460 | 662025 | 1 | EACH | MANHOLE TYPE C-6' DIAMETER OVER 14' TO 18' DEPTH |  | S100682 |
| 470 | 663049 | 1 | LS | PRECONSTRUCTION UTILITY SURVEY |  | S100682 |
| 480 | 664000 | 1 | LS | LANDSCAPE, COMPLETE |  | S100682 |
| 490 | 664010 | 1 | LS | GREEN STORMWATER INFRASTRUCTURE |  | S100682 |
| 500 | 664100 | 1 | LS | TEMPORARY TREE AND PLANT PROTECTION COMPLETE |  | S100682 |
| 510 | 664480 | 1 | LS | LANDSCAPE SEEDING COMPLETE |  | S100682 |
| 520 | 664995 | 1 | LS | IRRIGATION SYSTEM COMPLETE |  | S100682 |
| 530 | 701030 | 24 | EACH | REMOVE AND RESET PANEL SIGN |  | S100682 |
| 540 | 701100 | 315 | L.F. | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS |  | S100682 |
| 550 | 702000 | 100 | S.F. | CONSTRUCTION SIGNING |  | S100682 |
| 560 | 702100 | 140 | L.F. | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING |  | S100682 |
| 570 | 702220 | 5 | EACH | BARRICADE, TYPE II |  | S100682 |
| 580 | 702238 | 6 | EACH | BARRICADE, TYPE III-8' |  | S100682 |
| 590 | 702525 | 30 | EACH | CHANNELIZATION DEVICES TYPE DRUM |  | S100682 |
| 600 | 702610 | 2 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  | S100682 |
| 610 | 704000 | 11100 | L.F. | RETROREFLECTORIZED PAINTED MARKINGS 4" |  | S100682 |
| 620 | 704704 | 700 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKING 24" |  | S100682 |
| 630 | 704933 | 9 | EACH | PREFORMED THERMOPLASTIC PAVEMENT MARKING HANDICAPPED SYMBOL |  | S100682 |
| 640 | 707810 | 2 | EACH | REMOVE & RESET LIGHTING STANDARD & LUMINAIRE |  | S100682 |
| 650 | 709020 | 280 | L.F. | RIGID ELECTRICAL CONDUIT 2" (DIA.) |  | S100682 |
| 660 | 710000 | 1 | EACH | ELECTRICAL PULL BOX (STANDARD) |  | S100682 |
| 670 | 711102 | 560 | L.F. | SINGLE CONDUCTOR 2 |  | S100682 |
| 680 | 801000 | 1 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  | S100682 |
| 690 | 802000 | 1 | LS | POST CONSTRUCTION PLANS | 20000 | S100682 |