|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Line | Item | Quantity | Unit | Description | Price | Proposal |
| 10 | 201000 | 1 | LS | CLEARING AND GRUBBING |  | 2100742 |
| 20 | 203000 | 75800 | C.Y. | UNCLASSIFIED EXCAVATION |  | 2100742 |
| 30 | 203100 | 100 | C.Y. | BORROW |  | 2100742 |
| 40 | 203211 | 45900 | S.Y. | UNSTABLE SUBGRADE STABILIZATION |  | 2100742 |
| 50 | 207000 | 309400 | S.Y. | SUBGRADE PREPARATION |  | 2100742 |
| 60 | 303000 | 115600 | TON | BASE COURSE |  | 2100742 |
| 70 | 403701 | 8350 | TON | OPEN GRADED FRICTION COURSE COMPLETE |  | 2100742 |
| 80 | 405000 | 89400 | S.Y. | DETOUR PAVEMENT CONSTRUCTION |  | 2100742 |
| 90 | 407000 | 289 | TON | ASPHALT MATERIAL FOR TACK COAT |  | 2100742 |
| 100 | 408100 | 511 | TON | PRIME COAT MATERIAL |  | 2100742 |
| 110 | 414000 | 144300 | SYIN | COLD MILLING (ASPHALT) |  | 2100742 |
| 120 | 416207 | 10450 | S.Y. | MINOR PAVING TYPE II, HMA SP-IV |  | 2100742 |
| 130 | 423283 | 120380 | TON | HMA SP-IV COMPLETE |  | 2100742 |
| 140 | 511000 | 160 | C.Y. | STRUCTURAL CONCRETE, CLASS A |  | 2100742 |
| 150 | 541200 | 6820 | LB | STRUCTURAL STEEL FOR MISCELLANEOUS STRUCTURES |  | 2100742 |
| 160 | 570018 | 10 | L.F. | 18" CULVERT PIPE |  | 2100742 |
| 170 | 570019 | 1 | EACH | 18" CULVERT PIPE END SECTION |  | 2100742 |
| 180 | 570024 | 216 | L.F. | 24" CULVERT PIPE |  | 2100742 |
| 190 | 570160 | 940 | L.F. | 35"SX24"R (NOMINAL) CULVERT PIPE ARCH |  | 2100742 |
| 200 | 601000 | 1 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  | 2100742 |
| 210 | 601110 | 191130 | S.Y. | REMOVAL OF SURFACING |  | 2100742 |
| 220 | 602000 | 10 | C.Y. | RIPRAP CLASS A |  | 2100742 |
| 230 | 603100 | 33 | ACRE | TEMPORARY SOIL STABILANT |  | 2100742 |
| 240 | 603262 | 5200 | L.F. | COMPOSTED MULCH SOCKS |  | 2100742 |
| 250 | 603281 | 1 | LS | SWPPP PLAN PREPARATION AND MAINTENANCE |  | 2100742 |
| 260 | 606598 | 600 | L.F. | TCWB RETAINED BY THE CONTRACTOR |  | 2100742 |
| 270 | 606599 | 1800 | L.F. | RESETTING OF TCWB |  | 2100742 |
| 280 | 613000 | 1 | LS | CLEANING CULVERTS AND DRAINAGE STRUCTURES |  | 2100742 |
| 290 | 618000 | 1 | LS | TRAFFIC CONTROL MANAGEMENT |  | 2100742 |
| 300 | 618011 | 1 | LS | PUBLIC AWARENESS | 100000 | 2100742 |
| 310 | 621000 | 1 | LS | MOBILIZATION |  | 2100742 |
| 320 | 631000 | 142700 | L.F. | RUMBLE STRIPS |  | 2100742 |
| 330 | 632000 | 27 | ACRE | CLASS A SEEDING |  | 2100742 |
| 340 | 663049 | 1 | LS | PRECONSTRUCTION UTILITY SURVEY |  | 2100742 |
| 350 | 701000 | 1040 | S.F. | PANEL SIGNS |  | 2100742 |
| 360 | 701030 | 2 | EACH | REMOVE AND RESET PANEL SIGN |  | 2100742 |
| 370 | 701100 | 2500 | L.F. | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS |  | 2100742 |
| 380 | 701101 | 3 | EACH | MULTI-DIRECTIONAL SLIP BASE POSTS FOR ALUMINUM PANEL SIGNS |  | 2100742 |
| 390 | 702000 | 2608 | S.F. | CONSTRUCTION SIGNING |  | 2100742 |
| 400 | 702100 | 4034 | L.F. | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING |  | 2100742 |
| 410 | 702101 | 30 | EACH | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING |  | 2100742 |
| 420 | 702110 | 41 | EACH | PORTABLE SIGN SUPPORT |  | 2100742 |
| 430 | 702238 | 5 | EACH | BARRICADE, TYPE III-8' |  | 2100742 |
| 440 | 702320 | 303 | EACH | VERTICAL PANEL, TYPE BACK TO BACK |  | 2100742 |
| 450 | 702525 | 604 | EACH | CHANNELIZATION DEVICES TYPE DRUM |  | 2100742 |
| 460 | 702610 | 4 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  | 2100742 |
| 470 | 702850 | 1 | ALOW | LAW ENFORCEMENT IN CONSTRUCTION ZONE | 15000 | 2100742 |
| 480 | 703100 | 45 | EACH | ROAD DELINEATOR TYPE GUIDE |  | 2100742 |
| 490 | 704000 | 601300 | L.F. | RETROREFLECTORIZED PAINTED MARKINGS 4" |  | 2100742 |
| 500 | 704099 | 765100 | L.F. | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" |  | 2100742 |
| 510 | 704735 | 12 | EACH | HOT THERMOPLASTIC PAVEMENT MARKING RIGHT LANE DROP ARROW |  | 2100742 |
| 520 | 704875 | 2600 | EACH | TEMPORARY REFLECTIVE RAISED PAVEMENT MARKER, TYPE TD |  | 2100742 |
| 530 | 704876 | 1800 | EACH | TEMPORARY REFLECTIVE RAISED PAVEMENT MARKER, TYPE TG |  | 2100742 |
| 540 | 720060 | 2 | EACH | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES |  | 2100742 |
| 550 | 720110 | 6 | EACH | REMOVE/RESET IMPACT ATTENUATOR UNIT |  | 2100742 |
| 560 | 721000 | 526200 | L.F. | REMOVAL OF PAVEMENT MARKING |  | 2100742 |
| 570 | 801000 | 1 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  | 2100742 |
| 580 | 802000 | 1 | LS | POST CONSTRUCTION PLANS | 15000 | 2100742 |
| 590 | 802010 | 1 | LS | CAMP DATA COLLECTION |  | 2100742 |
|  |  |  |  |  |  |  |