|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Line | Item | Quantity | Unit | Description | Price | Proposal |  |
| 10 | 203000 | 267 | C.Y. | UNCLASSIFIED EXCAVATION |  | A301001 |  |
| 20 | 210002 | 9335 | C.Y. | MAJOR STRUCTURE EXCAVATION |  | A301001 |  |
| 30 | 210003 | 8825 | C.Y. | MAJOR STRUCTURE BACKFILL |  | A301001 |  |
| 40 | 210010 | 1 | LS | TEMPORARY RETAINING WALL/SHORING |  | A301001 |  |
| 50 | 501090 | 3 | EACH | ADDITIONAL PILE SPLICES |  | A301001 |  |
| 60 | 501101 | 30 | L.F. | PILE CUT-OFFS |  | A301001 |  |
| 70 | 501116 | 2626 | L.F. | DRIVEN PILES (16" PIPE) |  | A301001 |  |
| 80 | 502048 | 860 | L.F. | DRILLED SHAFT FOUNDATION 48" DIAMETER |  | A301001 |  |
| 90 | 502060 | 5520 | L.F. | DRILLED SHAFT FOUNDATION 60" DIAMETER |  | A301001 |  |
| 100 | 502166 | 1800 | L.F. | PERMANENT CASING 66" DIAMETER |  | A301001 |  |
| 110 | 502600 | 638 | L.F. | OBSTRUCTION REMOVAL |  | A301001 |  |
| 120 | 504301 | 6 | EACH | PILE DYNAMIC TEST CONSULTANT TESTING |  | A301001 |  |
| 130 | 504401 | 12 | EACH | CASE PILE WAVE ANALYSIS TEST CONSULTANT TESTING |  | A301001 |  |
| 140 | 505000 | 14 | EACH | CROSSHOLE SONIC LOGGING CONSULTANT TESTING |  | A301001 |  |
| 150 | 505003 | 70 | EACH | THERMAL INTEGRITY PROFILING CONSULTANT TESTING |  | A301001 |  |
| 160 | 505011 | 14 | EACH | LOW STRAIN INTEGRITY CONSULTANT TESTING |  | A301001 |  |
| 170 | 506000 | 29640 | S.F. | MSE PANEL WALL |  | A301001 |  |
| 180 | 511000 | 6054 | C.Y. | STRUCTURAL CONCRETE, CLASS A |  | A301001 |  |
| 190 | 511070 | 5915 | C.Y. | STRUCTURAL CONCRETE, CLASS HPD |  | A301001 |  |
| 200 | 511200 | 136 | S.Y. | STRUCTURAL CONCRETE, CLASS A-4" |  | A301001 |  |
| 210 | 511601 | 1 | LS | WIND BREAK |  | A301001 |  |
| 220 | 511602 | 1 | LS | FOGGING SYSTEM |  | A301001 |  |
| 230 | 512008 | 52 | C.Y. | ULTRA HIGH PERFORMANCE CONCRETE |  | A301001 |  |
| 240 | 514042 | 3302 | L.F. | CONCRETE BARRIER RAILINGS 42" |  | A301001 |  |
| 250 | 536001 | 16304 | S.Y. | EPOXY URETHANE POLYMER CONCRETE BRIDGE DECK OVERLAY |  | A301001 |  |
| 260 | 540060 | 1685660 | LB | REINFORCING BARS GRADE 60 |  | A301001 |  |
| 270 | 540061 | 1512600 | LB | GALVANIZED BARS GRADE 60 |  | A301001 |  |
| 280 | 540170 | 1036 | EACH | MECHANICAL COUPLERS |  | A301001 |  |
| 290 | 541100 | 4267205 | LB | STRUCTURAL STEEL FOR STEEL BRIDGES |  | A301001 |  |
| 300 | 543100 | 3302 | L.F. | METAL RAILING, PEDESTRIAN |  | A301001 |  |
| 310 | 548001 | 136429 | S.F. | COATING OF CONCRETE - STAIN |  | A301001 |  |
| 320 | 560000 | 273 | EACH | ELASTOMERIC BEARING PADS |  | A301001 |  |
| 330 | 562000 | 778 | L.F. | BRIDGE JOINT STRIP SEAL |  | A301001 |  |
| 340 | 563099 | 438 | L.F. | POLYMER BRIDGE JOINT SEALS |  | A301001 |  |
| 350 | 564000 | 990 | L.F. | PREFORMED CLOSED CELL FOAM BRIDGE JOINT SEALS |  | A301001 |  |
| 360 | 570413 | 750 | L.F. | 12" STORM DRAIN CULVERT PIPE |  | A301001 |  |
| 370 | 570419 | 440 | L.F. | 15" STORM DRAIN CULVERT PIPE |  | A301001 |  |
| 380 | 570425 | 230 | L.F. | 18" STORM DRAIN CULVERT PIPE |  | A301001 |  |
| 390 | 601000 | 1 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  | A301001 |  |
| 400 | 601997 | 1 | C.Y. | AC-ABATEMENT |  | A301001 |  |
| 410 | 602000 | 1209 | C.Y. | RIPRAP CLASS A |  | A301001 |  |
| 420 | 602060 | 15 | S.Y. | RIPRAP CLASS G |  | A301001 |  |
| 430 | 602200 | 301 | C.Y. | GABIONS |  | A301001 |  |
| 440 | 604300 | 10799 | S.Y. | GEOGRID REINFORCEMENT |  | A301001 |  |
| 450 | 623200 | 1 | LS | DROP INLETS COMPLETE |  | A301001 |  |
| 460 | 635000 | 8 | EACH | BAT BOX |  | A301001 |  |
| 470 | 107000 | 1 | LS | ENVIRONMENTAL COMMITMENTS |  | A301001 |  |
| 480 | 201000 | 1 | LS | CLEARING AND GRUBBING |  | A301001 |  |
| 490 | 203000 | 33000 | C.Y. | UNCLASSIFIED EXCAVATION |  | A301001 |  |
| 500 | 203100 | 20000 | C.Y. | BORROW |  | A301001 |  |
| 510 | 203200 | 3000 | C.Y. | UNSUITABLE MATERIAL EXCAVATION |  | A301001 |  |
| 520 | 203211 | 6600 | S.Y. | UNSTABLE SUBGRADE STABILIZATION |  | A301001 |  |
| 530 | 206100 | 170 | C.Y. | SELECT BACKFILL MATERIAL |  | A301001 |  |
| 540 | 207000 | 47700 | S.Y. | SUBGRADE PREPARATION |  | A301001 |  |
| 550 | 210010 | 1 | LS | TEMPORARY RETAINING WALL/SHORING |  | A301001 |  |
| 560 | 303000 | 17500 | TON | BASE COURSE |  | A301001 |  |
| 570 | 303160 | 800 | S.Y. | BASE COURSE 6" |  | A301001 |  |
| 580 | 403705 | 1500 | TON | WARM MIX OPEN-GRADED FRICTION COURSE COMPLETE |  | A301001 |  |
| 590 | 405000 | 16000 | S.Y. | DETOUR PAVEMENT CONSTRUCTION |  | A301001 |  |
| 600 | 407000 | 42 | TON | ASPHALT MATERIAL FOR TACK COAT |  | A301001 |  |
| 610 | 407001 | 1 | TON | FOG SEAL |  | A301001 |  |
| 620 | 408100 | 88 | TON | PRIME COAT MATERIAL |  | A301001 |  |
| 630 | 416217 | 500 | S.Y. | MINOR PAVING TYPE II, WMA SP-IV |  | A301001 |  |
| 640 | 417000 | 4600 | S.Y. | MISCELLANEOUS PAVING |  | A301001 |  |
| 650 | 424004 | 19200 | TON | WMA SP-IV COMPLETE |  | A301001 |  |
| 660 | 450060 | 150 | S.Y. | CONCRETE PAVEMENT-6" |  | A301001 |  |
| 670 | 450100 | 120 | S.Y. | CONCRETE PAVEMENT-10" |  | A301001 |  |
| 680 | 502030 | 158 | L.F. | DRILLED SHAFT FOUNDATION 30" DIAMETER |  | A301001 |  |
| 690 | 511000 | 10 | C.Y. | STRUCTURAL CONCRETE, CLASS A |  | A301001 |  |
| 700 | 511030 | 250 | C.Y. | STRUCTURAL CONCRETE, CLASS AA |  | A301001 |  |
| 710 | 516000 | 150 | C.Y. | FLOWABLE FILL |  | A301001 |  |
| 720 | 540060 | 22950 | LB | REINFORCING BARS GRADE 60 |  | A301001 |  |
| 730 | 541200 | 8300 | LB | STRUCTURAL STEEL FOR MISCELLANEOUS STRUCTURES |  | A301001 |  |
| 740 | 570036 | 420 | L.F. | 36" CULVERT PIPE |  | A301001 |  |
| 750 | 570037 | 2 | EACH | 36" CULVERT PIPE END SECTION |  | A301001 |  |
| 760 | 570038 | 240 | L.F. | 36" CULVERT PIPE - SLIP LINING |  | A301001 |  |
| 770 | 570192 | 100 | L.F. | 128"SX83"R (NOMINAL) CULVERT PIPE ARCH |  | A301001 |  |
| 780 | 570437 | 2000 | L.F. | 24" STORM DRAIN CULVERT PIPE |  | A301001 |  |
| 790 | 570441 | 1 | EACH | 24" STORM DRAIN CULVERT PIPE END SECTION |  | A301001 |  |
| 800 | 570449 | 30 | L.F. | 30" STORM DRAIN CULVERT PIPE |  | A301001 |  |
| 810 | 570461 | 110 | L.F. | 36" STORM DRAIN CULVERT PIPE |  | A301001 |  |
| 820 | 570465 | 1 | EACH | 36" STORM DRAIN CULVERT PIPE END SECTION |  | A301001 |  |
| 830 | 570479 | 230 | L.F. | 54" STORM DRAIN CULVERT PIPE |  | A301001 |  |
| 840 | 570486 | 30 | L.F. | 60" STORM DRAIN CULVERT PIPE |  | A301001 |  |
| 850 | 570493 | 420 | L.F. | 66" STORM DRAIN CULVERT PIPE |  | A301001 |  |
| 860 | 570620 | 420 | L.F. | 28"SX18"R STORM DRAIN CPA |  | A301001 |  |
| 870 | 570623 | 10 | EACH | 28"SX18"R STORM DRAIN CPA END SECTION |  | A301001 |  |
| 880 | 601000 | 1 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  | A301001 |  |
| 890 | 601110 | 45700 | S.Y. | REMOVAL OF SURFACING |  | A301001 |  |
| 900 | 602000 | 70 | C.Y. | RIPRAP CLASS A |  | A301001 |  |
| 910 | 602110 | 350 | S.Y. | CONCRETE BLOCK REVETMENT |  | A301001 |  |
| 920 | 603051 | 1 | LS | CLEAN WATER ACT COMPLIANCE WORK PLAN |  | A301001 |  |
| 930 | 603100 | 11 | ACRE | TEMPORARY SOIL STABILANT |  | A301001 |  |
| 940 | 603262 | 2600 | L.F. | COMPOSTED MULCH SOCKS |  | A301001 |  |
| 950 | 603281 | 1 | LS | SWPPP PLAN PREPARATION AND MAINTENANCE |  | A301001 |  |
| 960 | 604002 | 740 | S.Y. | GEOTEXTILE CLASS 2 |  | A301001 |  |
| 970 | 606001 | 1212.5 | L.F. | SINGLE FACE W-BEAM GUARDRAIL |  | A301001 |  |
| 980 | 606542 | 4820 | L.F. | CONCRETE WALL BARRIER 42" |  | A301001 |  |
| 990 | 606595 | 270 | L.F. | CONCRETE WALL BARRIER (HALF SECTION) |  | A301001 |  |
| 1000 | 606598 | 10300 | L.F. | TCWB RETAINED BY THE CONTRACTOR |  | A301001 |  |
| 1010 | 606599 | 14000 | L.F. | RESETTING OF TCWB |  | A301001 |  |
| 1020 | 607004 | 1000 | L.F. | BARBED WIRE FENCE 4' |  | A301001 |  |
| 1030 | 607014 | 3000 | L.F. | WOVEN WIRE FENCE 4' |  | A301001 |  |
| 1040 | 607015 | 50 | EACH | BRACES/CORNER POSTS |  | A301001 |  |
| 1050 | 607026 | 900 | L.F. | CHAIN LINK FENCE 6' |  | A301001 |  |
| 1060 | 607079 | 4610 | L.F. | PEDESTRIAN/BICYCLE RAILING |  | A301001 |  |
| 1070 | 607199 | 40 | L.F. | REMOVE AND REBUILD FENCE |  | A301001 |  |
| 1080 | 607251 | 1 | EACH | REMOVE AND RESET GATE |  | A301001 |  |
| 1090 | 607312 | 2 | EACH | STANDARD GATE, 12' |  | A301001 |  |
| 1100 | 607496 | 1 | EACH | CHAIN LINK GATE, 12' SPAN X 6' RISE |  | A301001 |  |
| 1110 | 607512 | 5 | EACH | PIPE GATE 12' |  | A301001 |  |
| 1120 | 607514 | 3 | EACH | PIPE GATE 14' |  | A301001 |  |
| 1130 | 607518 | 4 | EACH | PIPE GATE 18' |  | A301001 |  |
| 1140 | 607995 | 3 | EACH | AMAFCA ACCESS CONTROL GATE |  | A301001 |  |
| 1150 | 607996 | 2 | EACH | AMAFCA EQUESTRIAN ACCESS |  | A301001 |  |
| 1160 | 608004 | 3870 | S.Y. | CONCRETE SIDEWALK 4" |  | A301001 |  |
| 1170 | 608106 | 160 | S.Y. | DRIVE PAD 6" |  | A301001 |  |
| 1180 | 608404 | 1600 | S.Y. | CONCRETE MEDIAN PAVEMENT 4" (COLORED AND PATTERNED) |  | A301001 |  |
| 1190 | 609200 | 800 | L.F. | HEADER CURB |  | A301001 |  |
| 1200 | 609205 | 110 | L.F. | CONCRETE CUT OFF WALL |  | A301001 |  |
| 1210 | 609318 | 8680 | L.F. | CONCRETE SLOPED CURB AND GUTTER 6" X 18" |  | A301001 |  |
| 1220 | 609324 | 120 | L.F. | CONCRETE SLOPED CURB AND GUTTER 6" X 24" |  | A301001 |  |
| 1230 | 609424 | 2680 | L.F. | CONCRETE VERTICAL CURB AND GUTTER TYPE B 6" X 24" |  | A301001 |  |
| 1240 | 609462 | 2980 | L.F. | CONCRETE VERTICAL CURB AND GUTTER TYPE C 8" X 32" |  | A301001 |  |
| 1250 | 609648 | 370 | L.F. | CONCRETE VALLEY GUTTER 6" X 48" |  | A301001 |  |
| 1260 | 609706 | 200 | L.F. | CONCRETE LAYDOWN CURB 6" |  | A301001 |  |
| 1270 | 613000 | 1 | LS | CLEANING CULVERTS AND DRAINAGE STRUCTURES |  | A301001 |  |
| 1280 | 617000 | 1 | LS | VIBRATION MONITORING |  | A301001 |  |
| 1290 | 618000 | 1 | LS | TRAFFIC CONTROL MANAGEMENT |  | A301001 |  |
| 1300 | 618011 | 1 | LS | PUBLIC AWARENESS | 100000 | A301001 |  |
| 1310 | 619212 | 1 | EACH | HEADGATE TYPE C-12" |  | A301001 |  |
| 1320 | 619624 | 2 | EACH | FLAPGATE 24" |  | A301001 |  |
| 1330 | 619630 | 1 | EACH | FLAPGATE 30" |  | A301001 |  |
| 1340 | 621000 | 1 | LS | MOBILIZATION |  | A301001 |  |
| 1350 | 623200 | 1 | LS | DROP INLETS COMPLETE |  | A301001 |  |
| 1360 | 623312 | 1 | EACH | CURB DROP INLET TYPE II-B, 0' TO 4' |  | A301001 |  |
| 1370 | 623401 | 6 | EACH | DROP INLET 4'X4'(TYPE I) H=4'-0" |  | A301001 |  |
| 1380 | 623404 | 2 | EACH | DROP INLET 4'X4' (TYPE I) H=4'-1" TO 6'-0" |  | A301001 |  |
| 1390 | 623407 | 1 | EACH | DROP INLET 4'X4' (TYPE I) H=6'-1" TO 8'-0" |  | A301001 |  |
| 1400 | 623410 | 4 | EACH | DROP INLET SPECIAL DESIGN |  | A301001 |  |
| 1410 | 632000 | 7 | ACRE | CLASS A SEEDING |  | A301001 |  |
| 1420 | 632010 | 1 | ACRE | CLASS B SEEDING |  | A301001 |  |
| 1430 | 632020 | 3 | ACRE | CLASS C SEEDING |  | A301001 |  |
| 1440 | 662000 | 3 | EACH | MANHOLE TYPE C-4' DIAMETER 0' TO 6' DEPTH |  | A301001 |  |
| 1450 | 662010 | 8 | EACH | MANHOLE TYPE C-6' DIAMETER 0' TO 6' DEPTH |  | A301001 |  |
| 1460 | 662040 | 2 | EACH | MANHOLE TYPE C-8' DIAMETER 0' TO 6' DEPTH |  | A301001 |  |
| 1470 | 662042 | 1 | EACH | MANHOLE TYPE C-8' DIAMETER OVER 6' TO 10' DEPTH |  | A301001 |  |
| 1480 | 662072 | 1 | EACH | MANHOLE TYPE E-6' DIAMETER OVER 6' TO 10' DEPTH |  | A301001 |  |
| 1490 | 662400 | 1 | EACH | MANHOLE ADJUSTMENT |  | A301001 |  |
| 1500 | 663049 | 1 | LS | PRECONSTRUCTION UTILITY SURVEY |  | A301001 |  |
| 1510 | 664000 | 1 | LS | LANDSCAPE, COMPLETE |  | A301001 |  |
| 1520 | 667110 | 4 | EACH | MAIL BOX INSTALLATION-SINGLE |  | A301001 |  |
| 1530 | 667210 | 8600 | S.Y. | LANDSCAPE GRAVEL |  | A301001 |  |
| 1540 | 668000 | 1 | LS | DEWATERING |  | A301001 |  |
| 1550 | 701000 | 500 | S.F. | PANEL SIGNS |  | A301001 |  |
| 1560 | 701030 | 4 | EACH | REMOVE AND RESET PANEL SIGN |  | A301001 |  |
| 1570 | 701100 | 600 | L.F. | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS |  | A301001 |  |
| 1580 | 702000 | 90 | S.F. | CONSTRUCTION SIGNING |  | A301001 |  |
| 1590 | 702100 | 150 | L.F. | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING |  | A301001 |  |
| 1600 | 702101 | 12 | EACH | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING | | A301001 |  |
| 1610 | 702527 | 230 | L.F. | LANE SEPARATOR SYSTEM |  | A301001 |  |
| 1620 | 702610 | 8 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  | A301001 |  |
| 1630 | 702700 | 1 | LS | TEMPORARY SIGNAL SPAN |  | A301001 |  |
| 1640 | 702710 | 1 | EACH | MOBILE TRAFFIC SIGNAL SYSTEM |  | A301001 |  |
| 1650 | 702810 | 1 | LS | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION |  | A301001 |  |
| 1660 | 702811 | 1 | LS | TRAFFIC CONTROL DEVICES FOR PEDESTRIAN AND BICYCLIST |  | A301001 |  |
| 1670 | 702850 | 1 | ALOW | LAW ENFORCEMENT IN CONSTRUCTION ZONE | 40000 | A301001 |  |
| 1680 | 703001 | 4 | EACH | OBJECT MARKER TYPE 1 |  | A301001 |  |
| 1690 | 703002 | 8 | EACH | OBJECT MARKER TYPE 2 |  | A301001 |  |
| 1700 | 703004 | 2 | EACH | OBJECT MARKER TYPE 4 |  | A301001 |  |
| 1710 | 704099 | 270000 | L.F. | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" |  | A301001 |  |
| 1720 | 704101 | 24 | EACH | TEMPORARY WORD OR SYMBOL |  | A301001 |  |
| 1730 | 704700 | 39600 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKINGS 4" |  | A301001 |  |
| 1740 | 704702 | 1800 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKINGS 8" |  | A301001 |  |
| 1750 | 704704 | 400 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKING 24" |  | A301001 |  |
| 1760 | 704714 | 1 | EACH | HOT THERMOPLASTIC PAVEMENT MARKING COMBINATION (LEFT, THRU, RIGHT) ARROW | | A301001 |  |
| 1770 | 704716 | 2 | EACH | HOT THERMOPLASTIC PAVEMENT MARKING COMBINATION (THRU AND LEFT) ARROW | | A301001 |  |
| 1780 | 704717 | 11 | EACH | HOT THERMOPLASTIC PAVEMENT MARKING RIGHT ARROW |  | A301001 |  |
| 1790 | 704718 | 16 | EACH | HOT THERMOPLASTIC PAVEMENT MARKING LEFT ARROW |  | A301001 |  |
| 1800 | 704720 | 15 | EACH | HOT THERMOPLASTIC PAVEMENT MARKING WORD (ONLY) |  | A301001 |  |
| 1810 | 704728 | 15 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKING YIELD LINE |  | A301001 |  |
| 1820 | 704859 | 10 | EACH | REFLECTIVE RAISED PAVEMENT MARKER TYPE H |  | A301001 |  |
| 1830 | 704904 | 1200 | L.F. | PREFORMED THERMOPLASTIC PAVEMENT MARKING 24" |  | A301001 |  |
| 1840 | 705000 | 1 | ALOW | SIGNAL/LIGHTING SYSTEM START-UP COSTS | 12000 | A301001 |  |
| 1850 | 706100 | 2 | EACH | SERVICE RISER (SIGNAL) |  | A301001 |  |
| 1860 | 706110 | 2 | EACH | SERVICE RISER (LIGHTING) |  | A301001 |  |
| 1870 | 706200 | 2 | EACH | METER PEDESTAL (SIGNAL) |  | A301001 |  |
| 1880 | 706350 | 1 | LS | POWER SERVICE INSTALLATION | 70000 | A301001 |  |
| 1890 | 706405 | 1 | EACH | LIGHTING CONTROL CABINET-SIX CIRCUIT |  | A301001 |  |
| 1900 | 706420 | 1 | EACH | LIGHTING CONTROL CABINET-TWO CIRCUIT |  | A301001 |  |
| 1910 | 707540 | 62 | EACH | TYPE V STANDARD, 40' |  | A301001 |  |
| 1920 | 707742 | 3 | EACH | TYPE V STANDARD, 40', 2 ARMS |  | A301001 |  |
| 1930 | 707810 | 1 | EACH | REMOVE & RESET LIGHTING STANDARD & LUMINAIRE |  | A301001 |  |
| 1940 | 709020 | 12200 | L.F. | RIGID ELECTRICAL CONDUIT 2" (DIA.) |  | A301001 |  |
| 1950 | 709030 | 100 | L.F. | RIGID ELECTRICAL CONDUIT 3" (DIA.) |  | A301001 |  |
| 1960 | 710000 | 11 | EACH | ELECTRICAL PULL BOX (STANDARD) |  | A301001 |  |
| 1970 | 710010 | 1 | EACH | ELECTRICAL PULL BOX (LARGE) |  | A301001 |  |
| 1980 | 710200 | 12 | EACH | METAL PULL BOX |  | A301001 |  |
| 1990 | 711102 | 24200 | L.F. | SINGLE CONDUCTOR 2 |  | A301001 |  |
| 2000 | 711106 | 12600 | L.F. | SINGLE CONDUCTOR 6 |  | A301001 |  |
| 2010 | 711220 | 180 | L.F. | SINGLE CONDUCTOR 2/0 |  | A301001 |  |
| 2020 | 711240 | 150 | L.F. | SINGLE CONDUCTOR 4/0 |  | A301001 |  |
| 2030 | 716701 | 65 | EACH | LED ROADWAY LUMINAIRE |  | A301001 |  |
| 2040 | 720050 | 2 | EACH | PERMANENT VEHICULAR IMPACT ATTENUATOR UNIT |  | A301001 |  |
| 2050 | 720060 | 7 | EACH | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES |  | A301001 |  |
| 2060 | 720110 | 16 | EACH | REMOVE/RESET IMPACT ATTENUATOR UNIT |  | A301001 |  |
| 2070 | 721000 | 73000 | L.F. | REMOVAL OF PAVEMENT MARKING |  | A301001 |  |
| 2080 | 721101 | 40 | EACH | REMOVAL OF PAVEMENT MARKING SYMBOL |  | A301001 |  |
| 2090 | 730101 | 1 | LS | CONTINUOUS COUNT STATIONS |  | A301001 |  |
| 2100 | 750000 | 1 | LS | INTELLIGENT TRANSPORTATION SYSTEM |  | A301001 |  |
| 2110 | 750024 | 27200 | L.F. | COMMUNICATIONS CONDUIT 4" |  | A301001 |  |
| 2120 | 750032 | 6900 | L.F. | MULTI-DUCT CONDUIT 2" (8-WAY) |  | A301001 |  |
| 2130 | 750060 | 4 | EACH | ITS PULLBOX (33"X24"X24") |  | A301001 |  |
| 2140 | 750080 | 3 | EACH | ITS MANHOLE (48"X48"X48") |  | A301001 |  |
| 2150 | 750090 | 4 | EACH | ITS MANHOLE (76"X76"X71") |  | A301001 |  |
| 2160 | 750100 | 2 | EACH | CLOSED CIRCUIT TELEVISION SYSTEM (CCTV) |  | A301001 |  |
| 2170 | 750110 | 4 | EACH | CAMERA LOWERING DEVICE |  | A301001 |  |
| 2180 | 750150 | 2 | EACH | ITS STEEL POLE, 50 FT |  | A301001 |  |
| 2190 | 801000 | 1 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  | A301001 |  |
| 2200 | 802000 | 1 | LS | POST CONSTRUCTION PLANS | 50000 | A301001 |  |
| 2210 | 802010 | 1 | LS | CAMP DATA COLLECTION |  | A301001 |  |
| 2220 | 803000 | 1 | LS | SCHEDULE SOFTWARE |  | A301001 |  |
| 2230 | 803010 | 1 | LS | CPM TRAINING |  | A301001 |  |
| 2240 | 803020 | 1 | LS | CPM HARDWARE/EQUIPMENT |  | A301001 |  |