|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Line | Item | Quantity | Unit | Description | Price | Proposal |
| 0010 | 210003 | 690 | C.Y. | MAJOR STRUCTURE BACKFILL |  | 6101001 |
| 0020 | 502042 | 360 | L.F. | DRILLED SHAFT FOUNDATION 42" DIAMETER |  | 6101001 |
| 0030 | 502060 | 210 | L.F. | DRILLED SHAFT FOUNDATION 60" DIAMETER |  | 6101001 |
| 0040 | 502166 | 90 | L.F. | PERMANENT CASING 66" DIAMETER |  | 6101001 |
| 0050 | 502600 | 87 | L.F. | OBSTRUCTION REMOVAL |  | 6101001 |
| 0060 | 505001 | 12 | EACH | CROSSHOLE SONIC LOGGING DEPARTMENT TESTING |  | 6101001 |
| 0070 | 505010 | 12 | EACH | LOW STRAIN INTEGRITY DEPARTMENT TESTING |  | 6101001 |
| 0080 | 511000 | 394 | C.Y. | STRUCTURAL CONCRETE, CLASS A |  | 6101001 |
| 0090 | 511070 | 612 | C.Y. | STRUCTURAL CONCRETE, CLASS HPD |  | 6101001 |
| 0100 | 511601 | 1 | LS | WIND BREAK |  | 6101001 |
| 0110 | 511602 | 1 | LS | FOGGING SYSTEM |  | 6101001 |
| 0120 | 518055 | 780 | L.F. | PRESTRESSED CONCRETE BRIDGE MEMBER TYPE BT-54 |  | 6101001 |
| 0130 | 518063 | 650 | L.F. | PRESTRESSED CONCRETE BRIDGE MEMBER TYPE 63 |  | 6101001 |
| 0140 | 536001 | 1510 | S.Y. | EPOXY URETHANE POLYMER CONCRETE BRIDGE DECK OVERLAY |  | 6101001 |
| 0150 | 540060 | 157950 | LB | REINFORCING BARS GRADE 60 |  | 6101001 |
| 0160 | 540061 | 122010 | LB | GALVANIZED BARS GRADE 60 |  | 6101001 |
| 0170 | 541000 | 13140 | LB | STRUCTURAL STEEL FOR CONCRETE BRIDGES |  | 6101001 |
| 0180 | 543002 | 663 | L.F. | METAL RAILING, TYPE A42 |  | 6101001 |
| 0190 | 560000 | 30 | EACH | ELASTOMERIC BEARING PADS |  | 6101001 |
| 0200 | 562000 | 116 | L.F. | BRIDGE JOINT STRIP SEAL |  | 6101001 |
| 0210 | 563099 | 111 | L.F. | POLYMER BRIDGE JOINT SEALS |  | 6101001 |
| 0220 | 601000 | 1 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  | 6101001 |
| 0230 | 604002 | 600 | S.Y. | GEOTEXTILE CLASS 2 |  | 6101001 |
| 0240 | 604300 | 2920 | S.Y. | GEOGRID REINFORCEMENT |  | 6101001 |
| 0250 | 607076 | 655 | L.F. | PEDESTRIAN SCREENING FENCE, TYPE 1 |  | 6101001 |
| 0260 | 201000 | 1 | LS | CLEARING AND GRUBBING |  | 6101001 |
| 0270 | 203000 | 60120 | C.Y. | UNCLASSIFIED EXCAVATION |  | 6101001 |
| 0280 | 203100 | 138735 | C.Y. | BORROW |  | 6101001 |
| 0290 | 203211 | 3230 | S.Y. | UNSTABLE SUBGRADE STABILIZATION |  | 6101001 |
| 0300 | 207000 | 19945 | S.Y. | SUBGRADE PREPARATION |  | 6101001 |
| 0310 | 213000 | 0.6 | MILE | OBLITERATING OLD ROAD |  | 6101001 |
| 0320 | 303000 | 5620 | TON | BASE COURSE |  | 6101001 |
| 0330 | 403701 | 81 | TON | OPEN GRADED FRICTION COURSE COMPLETE |  | 6101001 |
| 0340 | 405000 | 810 | S.Y. | DETOUR PAVEMENT CONSTRUCTION |  | 6101001 |
| 0350 | 407000 | 9 | TON | ASPHALT MATERIAL FOR TACK COAT |  | 6101001 |
| 0360 | 408100 | 26 | TON | PRIME COAT MATERIAL |  | 6101001 |
| 0370 | 414000 | 5470 | SYIN | COLD MILLING (ASPHALT) |  | 6101001 |
| 0380 | 416103 | 1275 | TON | MINOR PAVING TYPE I, HMA SP-III |  | 6101001 |
| 0390 | 416104 | 4365 | TON | MINOR PAVING TYPE I, HMA SP-IV |  | 6101001 |
| 0400 | 416204 | 510 | TON | MINOR PAVING TYPE II, HMA SP-IV |  | 6101001 |
| 0410 | 511000 | 5 | C.Y. | STRUCTURAL CONCRETE, CLASS A |  | 6101001 |
| 0420 | 515000 | 35 | C.Y. | REINF.CONCRETE FOR MINOR STRUCTURES |  | 6101001 |
| 0430 | 516000 | 68 | C.Y. | FLOWABLE FILL |  | 6101001 |
| 0440 | 570024 | 340 | L.F. | 24" CULVERT PIPE |  | 6101001 |
| 0450 | 570025 | 2 | EACH | 24" CULVERT PIPE END SECTION |  | 6101001 |
| 0460 | 570030 | 370 | L.F. | 30" CULVERT PIPE |  | 6101001 |
| 0470 | 570031 | 3 | EACH | 30" CULVERT PIPE END SECTION |  | 6101001 |
| 0480 | 601000 | 1 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  | 6101001 |
| 0490 | 601110 | 730 | S.Y. | REMOVAL OF SURFACING |  | 6101001 |
| 0500 | 602000 | 260 | C.Y. | RIPRAP CLASS A |  | 6101001 |
| 0510 | 602060 | 8870 | S.Y. | RIPRAP CLASS G |  | 6101001 |
| 0520 | 603100 | 23 | ACRE | TEMPORARY SOIL STABILANT |  | 6101001 |
| 0530 | 603262 | 10000 | L.F. | COMPOSTED MULCH SOCKS |  | 6101001 |
| 0540 | 603281 | 1 | LS | SWPPP PLAN PREPARATION AND MAINTENANCE |  | 6101001 |
| 0550 | 606001 | 600 | L.F. | SINGLE FACE W-BEAM GUARDRAIL |  | 6101001 |
| 0560 | 606051 | 2 | EACH | END TREATMENT TL-3 END TERMINAL |  | 6101001 |
| 0570 | 606053 | 2 | EACH | END TREATMENT W-BEAM END ANCHOR |  | 6101001 |
| 0580 | 606062 | 4 | EACH | TRANSITION METAL BARRIER TO RIGID BARRIER |  | 6101001 |
| 0590 | 606610 | 1040 | L.F. | TCWB RETAINED BY THE CONTRACTOR (10') |  | 6101001 |
| 0600 | 607014 | 3500 | L.F. | WOVEN WIRE FENCE 4' |  | 6101001 |
| 0610 | 607015 | 15 | EACH | BRACES/CORNER POSTS |  | 6101001 |
| 0620 | 607916 | 1 | EACH | BARBED WIRE GATE 16' |  | 6101001 |
| 0630 | 610000 | 32 | L.F. | CATTLE GUARD |  | 6101001 |
| 0640 | 613000 | 1 | LS | CLEANING CULVERTS AND DRAINAGE STRUCTURES |  | 6101001 |
| 0650 | 618000 | 1 | LS | TRAFFIC CONTROL MANAGEMENT |  | 6101001 |
| 0660 | 618011 | 1 | LS | PUBLIC AWARENESS | 15000 | 6101001 |
| 0670 | 621000 | 1 | LS | MOBILIZATION |  | 6101001 |
| 0680 | 622002 | 1 | EACH | FIELD LABORATORY, TYPE II |  | 6101001 |
| 0690 | 622110 | 1 | EACH | SUPPLEMENTAL HOT-MIX ASPHALT FIELD LABORATORY |  | 6101001 |
| 0700 | 623012 | 1 | EACH | MEDIAN DROP INLET TYPE I (RURAL) H=3'1" TO 6'0" |  | 6101001 |
| 0710 | 631000 | 3050 | L.F. | RUMBLE STRIPS |  | 6101001 |
| 0720 | 632000 | 16 | ACRE | CLASS A SEEDING |  | 6101001 |
| 0730 | 632010 | 2 | ACRE | CLASS B SEEDING |  | 6101001 |
| 0740 | 632020 | 1 | ACRE | CLASS C SEEDING |  | 6101001 |
| 0750 | 690001 | 1 | ALOW | RAILWAY FLAGGING | 500000 | 6101001 |
| 0760 | 701000 | 115 | S.F. | PANEL SIGNS |  | 6101001 |
| 0770 | 701100 | 265 | L.F. | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS |  | 6101001 |
| 0780 | 702000 | 100 | S.F. | CONSTRUCTION SIGNING |  | 6101001 |
| 0790 | 702100 | 120 | L.F. | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING |  | 6101001 |
| 0800 | 702101 | 6 | EACH | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING | | 6101001 |
| 0810 | 702610 | 2 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  | 6101001 |
| 0820 | 702810 | 1 | LS | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION |  | 6101001 |
| 0830 | 704099 | 28375 | L.F. | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" |  | 6101001 |
| 0840 | 704700 | 21750 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKINGS 4" |  | 6101001 |
| 0850 | 704704 | 85 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKING 24" |  | 6101001 |
| 0860 | 704706 | 405 | L.F. | HOT THERMOPLASTIC PAVEMENT MARKINGS 12" |  | 6101001 |
| 0870 | 704718 | 2 | EACH | HOT THERMOPLASTIC PAVEMENT MARKING LEFT ARROW |  | 6101001 |
| 0880 | 704720 | 1 | EACH | HOT THERMOPLASTIC PAVEMENT MARKING WORD (ONLY) |  | 6101001 |
| 0890 | 720060 | 4 | EACH | VEHICULAR IMPACT ATTENUATOR UNIT-WORK ZONES |  | 6101001 |
| 0900 | 721000 | 33100 | L.F. | REMOVAL OF PAVEMENT MARKING |  | 6101001 |
| 0910 | 801000 | 1 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  | 6101001 |
| 0920 | 802000 | 1 | LS | POST CONSTRUCTION PLANS | 36000 | 6101001 |
| 0930 | 802010 | 1 | LS | CAMP DATA COLLECTION |  | 6101001 |
| 0940 | 803000 | 1 | LS | SCHEDULE SOFTWARE |  | 6101001 |
| 0950 | 803020 | 1 | LS | CPM HARDWARE/EQUIPMENT |  | 6101001 |