|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Line | Item | Quantity | Unit | Description | Price | Proposal |
| 10 | 201000 | 1 | LS | CLEARING AND GRUBBING |  | 5101870 |
| 20 | 203000 | 10500 | C.Y. | UNCLASSIFIED EXCAVATION |  | 5101870 |
| 30 | 203100 | 5300 | C.Y. | BORROW |  | 5101870 |
| 40 | 203211 | 6870 | S.Y. | UNSTABLE SUBGRADE STABILIZATION |  | 5101870 |
| 50 | 207000 | 27450 | S.Y. | SUBGRADE PREPARATION |  | 5101870 |
| 60 | 303000 | 10040 | TON | BASE COURSE |  | 5101870 |
| 70 | 403701 | 870 | TON | OPEN GRADED FRICTION COURSE COMPLETE |  | 5101870 |
| 80 | 407000 | 44 | TON | ASPHALT MATERIAL FOR TACK COAT |  | 5101870 |
| 90 | 408100 | 65 | TON | PRIME COAT MATERIAL |  | 5101870 |
| 100 | 414001 | 200 | S.Y. | COLD MILLING (ASPHALT) |  | 5101870 |
| 110 | 423282 | 21300 | TON | HMA SP-III COMPLETE |  | 5101870 |
| 120 | 502030 | 360 | L.F. | DRILLED SHAFT FOUNDATION 30" DIAMETER |  | 5101870 |
| 130 | 511030 | 100 | C.Y. | STRUCTURAL CONCRETE, CLASS AA |  | 5101870 |
| 140 | 540060 | 30491 | LB | REINFORCING BARS GRADE 60 |  | 5101870 |
| 150 | 570437 | 60 | L.F. | 24" STORM DRAIN CULVERT PIPE |  | 5101870 |
| 160 | 570441 | 1 | EACH | 24" STORM DRAIN CULVERT PIPE END SECTION |  | 5101870 |
| 170 | 601000 | 1 | LS | REMOVAL OF STRUCTURES AND OBSTRUCTIONS |  | 5101870 |
| 180 | 601110 | 19550 | S.Y. | REMOVAL OF SURFACING |  | 5101870 |
| 190 | 602060 | 700 | S.Y. | RIPRAP CLASS G |  | 5101870 |
| 200 | 603100 | 6 | ACRE | TEMPORARY SOIL STABILANT |  | 5101870 |
| 210 | 603262 | 600 | L.F. | COMPOSTED MULCH SOCKS |  | 5101870 |
| 220 | 603281 | 1 | LS | SWPPP PLAN PREPARATION AND MAINTENANCE |  | 5101870 |
| 230 | 606001 | 4775 | L.F. | SINGLE FACE W-BEAM GUARDRAIL |  | 5101870 |
| 240 | 606051 | 4 | EACH | END TREATMENT TL-3 END TERMINAL |  | 5101870 |
| 250 | 606053 | 4 | EACH | END TREATMENT W-BEAM END ANCHOR |  | 5101870 |
| 260 | 618000 | 1 | LS | TRAFFIC CONTROL MANAGEMENT |  | 5101870 |
| 270 | 618011 | 1 | LS | PUBLIC AWARENESS | 12500 | 5101870 |
| 280 | 621000 | 1 | LS | MOBILIZATION |  | 5101870 |
| 290 | 623012 | 1 | EACH | MEDIAN DROP INLET TYPE I (RURAL) H=3'1" TO 6'0" |  | 5101870 |
| 300 | 631000 | 6400 | L.F. | RUMBLE STRIPS |  | 5101870 |
| 310 | 632000 | 5 | ACRE | CLASS A SEEDING |  | 5101870 |
| 320 | 701000 | 310 | S.F. | PANEL SIGNS |  | 5101870 |
| 330 | 701030 | 2 | EACH | REMOVE AND RESET PANEL SIGN |  | 5101870 |
| 340 | 701040 | 1 | EACH | REMOVE AND RESET EXTRUDED PANEL SIGN |  | 5101870 |
| 350 | 701100 | 573 | L.F. | STEEL POST AND BASE POST FOR ALUMINUM PANEL SIGNS |  | 5101870 |
| 360 | 701108 | 24 | L.F. | STEEL I-BEAM POST TY S4X7.7 |  | 5101870 |
| 370 | 702000 | 200 | S.F. | CONSTRUCTION SIGNING |  | 5101870 |
| 380 | 702100 | 200 | L.F. | STEEL POSTS AND BASE POSTS FOR CONSTRUCTION SIGNING |  | 5101870 |
| 390 | 702101 | 12 | EACH | MULTI-DIRECTIONAL SLIP BASE POSTS FOR CONSTRUCTION SIGNING |  | 5101870 |
| 400 | 702610 | 4 | EACH | PORTABLE CHANGEABLE MESSAGE SIGN |  | 5101870 |
| 410 | 702810 | 1 | LS | TRAFFIC CONTROL DEVICES FOR CONSTRUCTION |  | 5101870 |
| 420 | 702850 | 1 | ALOW | LAW ENFORCEMENT IN CONSTRUCTION ZONE | 24350 | 5101870 |
| 430 | 704002 | 61600 | L.F. | RETROREFLECTORIZED PAINTED MARKINGS 6" |  | 5101870 |
| 440 | 704004 | 16100 | L.F. | RETROREFLECTORIZED PAINTED MARKINGS 12" |  | 5101870 |
| 450 | 704099 | 41600 | L.F. | TEMPORARY RETROREFLECTORIZED PAINTED MARKINGS 4" |  | 5101870 |
| 460 | 704735 | 6 | EACH | HOT THERMOPLASTIC PAVEMENT MARKING RIGHT LANE DROP ARROW |  | 5101870 |
| 470 | 704856 | 70 | EACH | REFLECTIVE RAISED PAVEMENT MARKER TYPE C |  | 5101870 |
| 480 | 704860 | 10 | EACH | REFLECTIVE RAISED PAVEMENT MARKER TYPE J |  | 5101870 |
| 490 | 704869 | 150 | EACH | PLOWABLE REFLECTIVE RAISED PAVEMENT MARKER TYPE PG |  | 5101870 |
| 500 | 707540 | 48 | EACH | TYPE V STANDARD, 40' |  | 5101870 |
| 510 | 709020 | 7950 | L.F. | RIGID ELECTRICAL CONDUIT 2" (DIA.) |  | 5101870 |
| 520 | 711102 | 16150 | L.F. | SINGLE CONDUCTOR 2 |  | 5101870 |
| 530 | 716701 | 48 | EACH | LED ROADWAY LUMINAIRE |  | 5101870 |
| 540 | 721000 | 34940 | L.F. | REMOVAL OF PAVEMENT MARKING |  | 5101870 |
| 550 | 801000 | 1 | LS | CONSTRUCTION STAKING BY THE CONTRACTOR |  | 5101870 |
| 560 | 802000 | 1 | LS | POST CONSTRUCTION PLANS | 5000 | 5101870 |
| 570 | 802010 | 1 | LS | CAMP DATA COLLECTION |  | 5101870 |
| 580 | 803000 | 1 | LS | SCHEDULE SOFTWARE |  | 5101870 |